|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sr. No.** | **Description** | **HSN NO.** | **Unit** | **Rate (RS)** |
| 1 | Providing and applying two coats of whitewash with approved quality white lime as specified on walls and ceilings etc., applied and brought to uniform finish, and preparation of surfaces complete all as per Engineer in Charge’s Instructions. | 2522 | Sq.m |  |
| 2 | Providing and applying two coats of acrylic distemper as specified on all walls and ceilings etc. applied and brought to uniform finish, over and including one coat of appropriate primer and preparation of surfaces complete all as per Manufacturer’s instructions. Make: Berger/ Asian. | 32099090 | Sq.m |  |
| 3 | Providing and applying two coats of acrylic distemper as specified on all walls and ceilings etc applied and brought to uniform finish, and preparation of surfaces complete all as per Manufacturer’s instructions. Make: Berger/Asian. | 32099090 | Sq.m |  |
| 4 | Providing and applying two coats of enamel paint as specified on walls etc applied and brought to uniform finish, over and including one coat of appropriate primer and preparation of surfaces complete all as per manufacturer’s instructions. Make: Berger/Asian. | 32081010 | Sq.m |  |
| 5 | Providing and applying two coats of acrylic emulsion paint as specified on all walls and ceilings etc applied and brought to uniform finish, over and including one coat of appropriate primer and preparation of surfaces complete all as per manufacturer’s instructions. Make: Berger/ Asian. | 32091010 | Sq.m |  |
| 6 | Providing and applying two coats of acrylic emulsion paint as specified on walls and ceilings etc applied and brought to uniform finish, and preparation of surfaces complete all as per manufacturer’s instructions. Make: Berger/Asian. | 32091010 | Sq.m |  |
| 7 | Providing and applying two coats of Velvet Touch Premium emulsion paint as specified on walls and ceilings etc applied and brought to uniform finish, over and including one coat of appropriate primer and preparation of surfaces complete all as per manufacturer’s instructions. Make: Berger/Asian. | 32091010 | Sq.m |  |
| 8 | Providing and applying two coats Enamel Paint of as specified on all doors, windows, ventilators, Window & Ventilators grills and staircase handrail surfaces etc applied and brought to uniform finish, over and including one coat of appropriate primer and preparation of surfaces complete all as per manufacturer’s instructions. Make: Burger/Asian. | 32081010 | Sq.m |  |
| 9 | Providing and applying two coats Enamel Paint as specified on all Doors, Windows, Ventilators, Window & Ventilators grills and staircase handrail surfaces etc applied and brought to uniform finish, and preparation of surfaces complete all as per manufacturer’s instructions. Make: Berger/Asian. | 32081010 | Sq.m |  |
| **Sr**. | **Description** | **HSN NO.** | **Unit** | **Rate (RS)** |
| 10 | Providing and applying two coats Enamel Paint exterior grade as specified on all doors, Windows, Ventilators, Window & Ventilators grills and staircase handrail surfaces etc. applied and brought to uniform finish, and preparation of surfaces complete all as per manufacturer’s instructions. Make: Berger/Asian. | 32081010 | Sq.m |  |
| 11 | Providing and applying two coats of cement-based paint as specified on all external walls applied and brought to uniform finish, and preparation and curing of surfaces complete all as per manufacturer’s instructions. Make: Berger/Asian | 3210 | Sq.m |  |
| 12 | Providing and applying two coats of Acrylic Exterior Paint as specified on external walls applied and brought to uniform finish, over and including one coat of appropriate primer and preparation of surfaces complete all as per manufacturer’s instructions. Make: Berger/Asian | 32091010 | Sq.m |  |
| 13 | Providing and applying two coats of Acrylic latex paint as specified on external walls applied and brought to uniform finish, over and including one coat of appropriate primer and preparation and curing of surfaces complete all as per manufacturer’s instructions. Make: Berger/Asian. | 32091010 | Sq.m |  |
| 14 | Providing and applying two coats of Putty as specified on walls, ceiling applied and brought to uniform finish, over and curing of surfaces complete all as per manufacturer’s instructions. Make: Birla/JK | 32141000 | Sq.m |  |